Things fixed from DFM analysis

* Via to close to pad
* Via to close to connector hole
* Traces too close to pad may be exposed by solder mask